/*******************************************************************************
*
* McStas, neutron ray-tracing package
*         Copyright (C) 1997-2006, All rights reserved
*         Risoe National Laboratory, Roskilde, Denmark
*         Institut Laue Langevin, Grenoble, France
*
* %I
* Written by:  Kim Lefmann
* Date: May 7, 2001
* Version: $Revision: 1.14 $
 Origin: Risoe
* Release: McStas 1.9.1
*
* Rectangular 1D PSD, measuring intensity vs. vertical position, x

* %D
*
* Example: PSDlin_monitor(nx=20, filename="Output.x",
*          xmin=-0.1, xmax=0.1, ymin=-0.1, ymax=0.1)
*
* %P
* INPUT PARAMETERS:
*
* xmin:     Lower x bound of detector opening (m)
* xmax:     Upper x bound of detector opening (m)
* ymin:     Lower y bound of detector opening (m)
* ymax:     Upper y bound of detector opening (m)
* xwidth:   Width/diameter of detector (x). Overrides xmin,xmax. (m)
* yheight:  Height of detector (y). Overrides ymin,ymax. (m)
* nx:       Number of x bins (1)
* filename: Name of file in which to store the detector image (text)
*
* OUTPUT PARAMETERS:
*
* PSDlin_N:    Array of neutron counts
* PSDlin_p:    Array of neutron weight counts
* PSDlin_p2:   Array of second moments
*
* %E
******************************************************************************/

DEFINE COMPONENT PSDlin_monitor
DEFINITION PARAMETERS (nx=20, filename)
SETTING PARAMETERS (xmin=0, xmax=0, ymin=0, ymax=0, xwidth=0, yheight=0)
OUTPUT PARAMETERS (PSDlin_N, PSDlin_p, PSDlin_p2)
STATE PARAMETERS (x,y,z,vx,vy,vz,t,s1,s2,p)
DECLARE
  %{
    double PSDlin_N[nx];
    double PSDlin_p[nx];
    double PSDlin_p2[nx];
  %}
INITIALIZE
  %{
    int i;

    if (xwidth  > 0) { xmax = xwidth/2;  xmin = -xmax; }
    if (yheight > 0) { ymax = yheight/2; ymin = -ymax; }

    if ((xmin >= xmax) || (ymin >= ymax)) {
            printf("PSDlin_monitor: %s: Null detection area !\n"
                   "ERROR           (xwidth,yheight,xmin,xmax,ymin,ymax). Exiting",
           NAME_CURRENT_COMP);
      exit(0);
    }

    for (i=0; i<nx; i++)
    {
      PSDlin_N[i] = 0;
      PSDlin_p[i] = 0;
      PSDlin_p2[i] = 0;
    }
  %}
TRACE
  %{
    int i;

    PROP_Z0;
    if (x>xmin && x<xmax && y>ymin && y<ymax)
    {
      i = floor(nx*(x-xmin)/(xmax-xmin));              /* Bin number */
      if((i >= nx) || (i<0))
      {
        printf("FATAL ERROR: wrong positioning in linear PSD. i= %i \n",i);
        exit(1);
      }
      PSDlin_N[i]++;
      PSDlin_p[i] += p;
      PSDlin_p2[i] += p*p;
    }
  %}
SAVE
  %{
    DETECTOR_OUT_1D(
        "Linear PSD monitor",
        "x-Position [m]",
        "Intensity",
        "x", xmin, xmax, nx,
        &PSDlin_N[0],&PSDlin_p[0],&PSDlin_p2[0],
        filename);
  %}

MCDISPLAY
%{
  magnify("xy");
  multiline(5, (double)xmin, (double)ymin, 0.0,
               (double)xmax, (double)ymin, 0.0,
               (double)xmax, (double)ymax, 0.0,
               (double)xmin, (double)ymax, 0.0,
               (double)xmin, (double)ymin, 0.0);
%}

END



