/*******************************************************************************
*
* McStas, neutron ray-tracing package
*         Copyright (C) 1997-2006, All rights reserved
*         Risoe National Laboratory, Roskilde, Denmark
*         Institut Laue Langevin, Grenoble, France
*
* Instrument: SANS_KWS2_NoSample
*
* %I
* Written by: Henrich Frielinghaus
* Date:       Sept 2004
* Origin:     FZ-Juelich/FRJ-2/IFF/KWS-2
* Version:    $Revision: 1.3 $
* Release:    McStas 1.9
* %INSTRUMENT_SITE: FZ_Juelich
*
* KWS2 SANS instrument at FZ-Juelich. No sample, 2 detectors.
*
* %D
*
* KWS2 SANS instrument at FZ-Juelich. No sample, 2 detectors.
*
* %P
* INPUT PARAMETERS:
* Lambda    : Mean wavelength of neutrons      [AA]
* D_lambda  : Wavelength spread of neutrons    [AA]
* r         : Radius of scattering hard spheres [AA]
* PHI       : Particle volume fraction [1]
* Delta_Rho : Excess scattering length density (fm/AA^3)
* Sigma_a   : Absorption cross section density at 2200 m/s [m^-1]
* Qmax      : Maximum momentum transfer [AA^-1]
*
* %E
*******************************************************************************/
DEFINE INSTRUMENT SANS_KWS2_NoSample(lam=7.0, dlam=0.7, FLUX=1e8,
     NGblen=0.05,
     Clen = 10.0, Dlen = 10.0,
     sampR=100.0, sampPhi=0.001, sampDrho=0.6, sampSigmaA=50.0, sampQmax=0.3)

TRACE

COMPONENT origin = Arm()
  AT (0,0,0) ABSOLUTE


COMPONENT source = Source_flux_lambda(
    radius = 1.414*NGblen, dist = Clen, xw = NGblen, yh = NGblen,
    lambda_0 = lam, d_lambda = dlam, flux = FLUX)
  AT (0, 0, 0) RELATIVE origin


COMPONENT guide = Guide(w1=NGblen, h1=NGblen, w2=NGblen, h2=NGblen, l=20.0,
                        R0=0.99, Qc=0.0219, alpha=6.07, m=2, W=0.003)
  AT (0, 0, Clen) RELATIVE source


COMPONENT Cguide= Guide(w1=NGblen, h1=NGblen, w2=NGblen, h2=NGblen, l=20.0-Clen,
                        R0=0.99, Qc=0.0219, alpha=6.07, m=2, W=0.003)
  AT (0, 0, 20) RELATIVE guide


COMPONENT SmpAp = Slit(xmin=-0.005, xmax=0.005,
                       ymin=-0.005, ymax=0.005)
  AT (0, 0, 19.95) RELATIVE Cguide


/*COMPONENT sample = Sans_spheres(R=sampR, Phi=sampPhi, Delta_rho=sampDrho, sigma_a=sampSigmaA,
                                qmax=sampQmax)
   AT (0,0, 20.00) RELATIVE Cguide
*/

COMPONENT sample = Arm()
   AT (0,0, 20.00) RELATIVE Cguide


/*COMPONENT Lmon = L_monitor(
    nchan = 1000, filename = "Lmon.dat",    xmin = -0.75*NGblen,
    xmax = 0.75*NGblen, ymin = -0.75*NGblen, ymax = 0.75*NGblen, Lmin = 4.5, Lmax = 12.5)
  AT (0, 0, Dlen-0.05) RELATIVE sample
*/

/*Component Bstop = Beamstop(xmin=-0.75*NGblen, xmax=0.75*NGblen,
                             ymin=-0.75*NGblen, ymax=0.75*NGblen)
  AT (0, 0, Dlen-0.005) RELATIVE sample
*/

COMPONENT detector = PSD_monitor(
    nx = 128, ny = 128, filename = "PSD.dat", xmin = -0.05,
    xmax = 0.05, ymin = -0.05, ymax = 0.05)
  AT (0, 0, Dlen) RELATIVE sample

COMPONENT detector2 = PSD_monitor_rad(rmax=0.07, nr=100, filename="PSDr.dat")
  AT (0, 0, 0.01) RELATIVE detector

END