/*******************************************************************************
*
* McStas, neutron ray-tracing package
*         Copyright (C) 1997-2006, All rights reserved
*         Risoe National Laboratory, Roskilde, Denmark
*         Institut Laue Langevin, Grenoble, France
*
* Instrument: SNS_test
*
* %Identification
* Written by: G. Granroth
* Date: July 2004
* Origin: SNS Project Oak Ridge National Laboratory
* %INSTRUMENT_SITE:tests
*
* %Description
* Simple test instrument for the SNS_source component.
* Refer to SNS <A href="http://www.sns.gov/users/instrument_systems/components/moderator/">Source files.</A>
*
* Example: mcrun SNS_test.instr
*
* %Link
* Written by G. Granroth
* SNS_source component
* <A href="http://www.sns.gov/users/instrument_systems/components/moderator/">Source files </A>
* %End
*******************************************************************************/

DEFINE INSTRUMENT SNS_test()

TRACE
COMPONENT mod=SNS_source(S_filename="source_sct091_tu_02_1.dat",
                         width=0.1,
                         height=0.12,
                         dist=1,
                         xw=0.10,
                         yh=0.24,
Emin=1.0,Emax=10.0)
AT(0,0,0) ABSOLUTE

COMPONENT dett=TOF_monitor(xmin = -.025,
	              xmax = .025,
		      ymin = -.06,
		      ymax = .06,
		      nchan=500,
                      dt=10,
                      filename="tout.det")
At (0,0,1) RELATIVE mod

COMPONENT det=Monitor_nD(
                      xmin = -.5,
	              xmax = .5,
		      ymin = -.5,
		      ymax = .5,
		      options=" square x bins 100 limits=[-0.05 0.05]; y bins 100 limits=[-0.12 0.12]")
AT (0,0,1.0000000000001) RELATIVE mod
END

